* Breaker type vibro-reduced
* Breaker version silenced
* Weight 27 kg
* Length 670 mm
* Air consumption 30 l/s
* Impact rate 1,320 blows/min
* Vibration level 3 axes (ISO 28927-10) 4.2 m/s²
* Sound power level guaranteed (2000/14/EC) 106 Lw. dB(A)
* Sound pressure level (ISO 11203) 93 Lp. dB(A)
* Shank size: Hex 28x160 mm - 1 1⁄8 x 61⁄4 inch
* Part number 8461 0225 34